One layer of brick flat soiling foundation or in floor with first class or picked jhama bricks including preparation of bed and filling the interstics with local sand, levelling etc. Complete and accepted by the Engineer.