#### Construction of brick wall

* Marking for brick walls & openings will be done on structural floor slab according to approved shop drawings.
* The floor slab where brick walls to be built will be cleaned.
* Reinforcement for stiffener columns will be anchored using HIT-HY 150 chemical at the place where Reinforcement starters would not be provided.
* Brick walls with 225mm thick will be built to around 1.5m height in first stage and balance will be completed after curing the wall.
* Brick walls with 112.5mm will be built to around 1.0m height in each curing.