250mm brick work in super structure wall with 1st class bricks in cement sand (F.M.-1.70) mortar of proportion 1:6 cement Akij / Holcem / Scan / Shah Special cement (1st one is 1st preferable if unavailable of 1st one than 2nd one & 3rd one will be used gradually) including screening and washing of sand, scaffolding staging, racking out joints, filling interstices with mortar cleaning and soaking out bricks at least 24 hours before use, curing at least 7 days and supplying af all materials etc. complete in all respect in all heights as per drawing, specification and direction of Engineer-in-Charge.