125mm thick brick work in 1st class bricks in cement sand (F.M.-1.70) mortar of proportion 1:4 Akij / Holcem / Scan / Shah Special cement (1st one is 1st preferable if unavailable of 1st one than 2nd one & 3rd one will be used gradually) cement (1st one is 1st preferable if unavailable of 1st one than 2nd one & 3rd one will be used gradually) providing bond with connected walls including screening and washing of sand, scaffolding, staging, racking out joints, soaking out bricks at least 24 hours before use, curing at least 7 days and supplying af all materials etc. complete in all respect in all heights as per drawing, specification and direction of Engineer-in-Charge.