25 mm thick patent stone and 20 mm thick cement sand (F.M. - 1.5) morter (1:3) base and racking out joints with repective joint fillar & binder including cutting, laying and hire charge of machine and finishing with care etc. for all floor RAK/Stair/Mir Ceramic/ approved Brand.