20 mm thick cement sand (F.M. 1.5) morter (1:3) base and racking out joints with repective joint fillar & binder including cutting, laying and hire charge of machine and finishing with care etc. 200 x 400 in sizes or equipment for all floor. RAK / Stair / Mir Ceramic / approved Brand.