Manufacturing supplying fitting and fixing of fixed glazed frame for all floors with outer member of 19 x 19 x 19 x 3 mm Z-section and vertical and horizontal dividers of 19 x 19 x3 mm T-section including all cost of fabrication and welding, supplying and fixing of 19 x 19 x3 mm angle clamps of 150 mm length (wih one end bifurcated) of required Nos. with the frame, fixing the frame in wall with (1:2:4) cement concrete in the hole for clamp after making necessary grooves, supplying and fixing of 3 mm glass panes with pucca putty, mending good all damages, painting iron face with two coats and synthtic enamel paint over a coat of anti-corrosive priming to approved colour and quality etc cost of electicity , workshop charges carrige etc all complete as per drawing and accepted by the Engineer. [Rate is excluding the cost of painting] (scope of work of this item is in staircase and over partition wall etc.).