Extra cost for concealing of G.I. / PVC pipe work (12mm & 25mm dia) in brick wall by cutting wall, lintel, beam etc, by any means carefully without damaging the structure & filling the grooves after laying of pipe with CC (4:2:1) including cost of scaffolding etc. all complete as per direction of the Engineer-in-charge.