Construction of sock well of different sizes (medium and large sizes) with 250 mm thick solid brick work and 250 mm honey comb brick work with cement mortar (1:6) as per design over R.C.C (1:2:4) well curb with 1% reinforcement up to the depth as per drawing with 450mm dia water sealed heavy type.C.I manhole cover with locking arrangement, filling the well up to the required depth with graded khoa and sand including supplying and fabrication M.S.rod, casting, curing including necessary earth work in excavation, side filling and bailling out water including cost of all materials etc.all complete as per drawing, design approved and accepted by the Engineer. (Rate is including cost of reinforcement and its fabrication, including cost of reinforcement and its fabrication, binding and placing), 200 Users Sock Well.