Providing and laying of following sizes LT PVC insulated sheaded and armoured cable (NYFGbY). All electrical contacts shall be of brass/copper connected through connector and cables shall be manufactured and tested according to relavent IEC/BDS/BS/VDE standards and as per detailed specification mentioned ia.Annexure-A. The work shall be carried out as per direction/approval/acceptance of the Engineer.  
In kutcha ground by cutting 45.7cm width x 91.4cm depth trench with necessary brick or file protection and mending the damages good by refilling trench with proper compection.