**Specification for mix design RCC of M20:**

Providing, mixing, placing in position, machine batched, machine mixed and machine vibrated design mix as per approved mix design RCC of M20 grade using 20mm downgraded stone-chips, sand of FM 2.5 and approved quality cement.