**Demolition and Removal of Asphalt Pavement:**

* Removal. Asphalt driveway removal can be accomplished using a jackhammer to break up the asphalt
* Debris is then removed.

**Preparing Sub-base for temporary road:**

* A subgrade soil must be compacted to an adequate density.
* Generally, adequate density is specified as a relative density for the top 150 mm (6 inches) of subgrade of not less than 95 percent of maximum density.
* Soil is to be compacted using frog hammer, 10 Kg / 20 Kg dormouse, plate vibrator and water spray at each 150 mm layer of soil. Final finish of the surface must be convex and wetted by water.