**Bituminous Painting:**

Road is needed to paint with hot bitumen at 178 to 188 degree Celsius and spreading it with iron rollers after perfectly cleaning road surface. After that sand should be spreader.