**Pipe transportation Procedure:**

1. The pipe, casing pipe, fittings all are stored in KAFCO Yard. One 11 ton crane will carry those pipes and placed in trolley with safety.
2. Trolley with tractor will carry those pipes, fittings and other bulk materials in the site with safety.
3. Shear leg with chain pulley will use for unloading those material and pipes near the trenching.
4. Lifting belt will be used for grapping the coated pipes.