***CONSTRUCTION PROCEDURE***

**Cutting and Transfer Old corroded pipe.**

Cutting:

1. Preparing trench for the corroded pipe.
2. Cutting the corroded pipe joint.
3. Setting Up the crane and tractor for pulling the cut corroded pipe from trench.
4. Transport the corroded pipe to required place.