**Pipe Laying Procedure:**

1. After finalizing of Pipe laying position on the trench, slipper has to be prepared.
2. Clearing of right of way has to be proper and shear leg has to be set properly
3. Trenching must be started before pipe transportation.
4. Welding joint has be completed and tested by KAFCO
5. Pipe hauling equipment has to be set and then with lifting belt the pipe will be lifted by chain pulley and shear leg.
6. Pipe will be lay on Slipper and sand bag have to provide on the trench.
7. After sequential joint on the trench with shear leg chain pulley pipe need to place on the trench.