Mass concrete (1:2:4) in foundation or floor having with cement Akij / Holcem / Scan / Shah Spocial cement (1st one is 1st preferable if unavailable of 1st one than 2nd one & 3rd one will be used gradually) sand (F,M.- 1.2) and picked jhama chips in/c. breaking chips screnning, centering, shuttering, mixing, laying, compacting to levels and curing for at least 7 days including the supply of water, electricity and other charges and cost of tools and plants etc. all complete and accepted by the Engineer.